NAESB WGQ Standard No. 0.4.z2 – Operational Capacity						R99033 et al Rec Revd Att 3

873 Commodity Movement Services

Functional Group ID=CU

Heading:

	Pos.	Seg.		Req.		Loop	
	No.	ID	Name	Des.	Max.Use	Repeat		
Must Use	0100	ST	Transaction Set Header	M	1									
Must Use	0200	BGN	Beginning Segment	M	1									
	0300	REF	Reference Information	O	>1									
Must Use	0400	DTM	Date/Time Reference	O	>1									
			LOOP ID - N1			>1								
Must Use	0500	N1	Party Identification	M	1									

Detail:

	Pos.	Seg.		Req.		Loop	
	No.	ID	Name	Des.	Max.Use	Repeat		
			LOOP ID - DTM			>1								
Must Use	0100	DTM	Date/Time Reference	M	1									
	0200	N9	Extended Reference Information	O	>1									
Must Use	0300	LQ	Industry Code Identification	O	>1									
	0450	MEA	Measurements	O	1									
Must Use	0470	QTY	Quantity Information	O	>1									
			LOOP ID - SLN			>1								
Must Use	0700	SLN	Subline Item Detail	O	1									
			LOOP ID - N1			>1								
Must Use	1100	N1	Party Identification	O	1									
	1200	LCD	Place/Location Description	O	1									
	1300	N9	Extended Reference Information	O	>1									
														
Must Use	1600	SE	Transaction Set Trailer	M	1									

	Segment:	ST Transaction Set Header
	Position:	0100
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	ST01	143	Transaction Set Identifier Code	M	1 	ID 3/3	
 	873		Commodity Movement Services	
Must Use	ST02	329	Transaction Set Control Number	M	1 	AN 4/9	

	Segment:	BGN Beginning Segment
	Position:	0200
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	BGN01	353	Transaction Set Purpose Code	M	1 	ID 2/2	
 	00		Original	
Must Use	BGN02	127	Reference Identification	M	1 	AN 1/80	
	The operational capacity tracking number assigned by the originator.  Send "N/A" if this identifier is not used.	
Must Use	BGN03	373	Date	M	1 	DT 8/8	
	The operational capacity issue date.	
Must Use	BGN07	640	Transaction Type Code	O	1 	ID 2/2	
 	OA		Operational Capacity	

	Segment:	REF Reference Information
	Position:	0300
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is sender's option.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	REF01	128	Reference Identification Qualifier	M	1 	ID 2/3	
 	L1		Letters or Notes	
Must Use	REF03	352	Description	X	1 	AN 1/80	
	Comments and Notes	

	Segment:	DTM Date/Time Reference
	Position:	0400
	Loop:
	Level:	Heading
	Usage:	Optional (Must Use)
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	DTM01	374	Date/Time Qualifier	M	1 	ID 3/3	
 	809		Posted	
Must Use	DTM05	1250	Date Time Period Format Qualifier	X	1 	ID 2/3	
 	DT		Date and Time Expressed in Format CCYYMMDDHHMM	
Must Use	DTM06	1251	Date Time Period	X	1 	AN 1/35	
	Posting Date, Posting Time	

	Segment:	N1 Party Identification
	Position:	0500
	Loop:	N1        Mandatory
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N101	98	Entity Identifier Code	M	1 	ID 2/3	
 	SJ		Service Provider	
Must Use	N103	66	Identification Code Qualifier	X	1 	ID 1/2	
	Parties should mutually agree to use the Transportation Service Provider's proprietary entity code when the D-U-N-S® Number is not available.	
 	1		D-U-N-S Number, Dun & Bradstreet	
	For NAESB WGQ, this code value may only be used when sending the Transportation Service Provider.	
 	SV		Service Provider Number	
	For NAESB WGQ, this code value may only be used when sending the Transportation Service Provider Proprietary Code.	
Must Use	N104	67	Identification Code	X	1 	AN 2/17	
	Transportation Service Provider/Transportation Service Provider Proprietary Code.

The data element maximum length is reduced from that which is specified in the ASC X12 standards.	

	Segment:	DTM Date/Time Reference
	Position:	0100
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	DTM01	374	Date/Time Qualifier	M	1 	ID 3/3	
 	007		Effective	
Must Use	DTM05	1250	Date Time Period Format Qualifier	X	1 	ID 2/3	
 	DT		Date and Time Expressed in Format CCYYMMDDHHMM	
Must Use	DTM06	1251	Date Time Period	X	1 	AN 1/35	
	Effective Gas Day, Effective Time	

	Segment:	N9 Extended Reference Information
	Position:	0200
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is sender's option.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N901	128	Reference Identification Qualifier	M	1 	ID 2/3	
	Refer to "N9 Segments (Detail)" table for usage and values.	
Must Use	N902	127	Reference Identification	X	1 	AN 1/80	
	Refer to "N9 Segments (Detail)" table for usage and values.

Comments and Notes, Cycle Indicator	

	Segment:	LQ Industry Code Identification
	Position:	0300
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LQ01	1270	Code List Qualifier Code	O	1 	ID 1/3	
	Refer to "LQ Segments (Detail)" table for usage and values.	
Must Use	LQ02	1271	Industry Code	X	1 	AN 1/30	
	Refer to "LQ Segments (Detail)" table for usage and values.

Flow Indicator, Location/Quantity Type Indicator, IT Indicator, Authorized Overrun Indicator	

	Segment:	MEA Measurements
	Position:	0450
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment is conditional.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	MEA02	738	Measurement Qualifier	O	1 	ID 1/3	
 	PU		Pressure Base	
Must Use	MEA03	739	Measurement Value	X	1 	R 1/20	
	Pressure Base	
	MEA04	C001	Composite Unit of Measure	X	1 		
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Pressure Base Indicator	
 	64		Pounds Per Square Inch Gauge	
 	80		Pounds Per Square Inch Absolute	

	Segment:	QTY Quantity Information
	Position:	0470
	Loop:	DTM        Mandatory
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	QTY01	673	Quantity Qualifier	M	1 	ID 2/2	
	Refer to "QTY Segments (Detail)" table for usage and values.	
Must Use	QTY02	380	Quantity	X	1 	R 1/15	
	Refer to "QTY Segments (Detail)" table for usage and values.

Operating Capacity, Operationally Available Capacity, Total Scheduled Quantity 	
	QTY03	C001	Composite Unit of Measure	O	1 		
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Measurement Basis	
 	BZ		Million BTU's	
 	G8		Gigacalories	
 	GV		Gigajoules	
 	TZ		Thousand Cubic Feet	

	Segment:	SLN Subline Item Detail
	Position:	0700
	Loop:	SLN        Optional (Must Use)
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	SLN01	350	Assigned Identification	M	1 	AN 1/20	
Must Use	SLN03	662	Relationship Code	M	1 	ID 1/1	
 	I		Included	

	Segment:	N1 Party Identification
	Position:	1100
	Loop:	N1        Optional (Must Use)
	Level:	Detail
	Usage:	Optional (Must Use)
	Max Use:	1
Notes:		For NAESB WGQ, this segment is mandatory.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N101	98	Entity Identifier Code	M	1 	ID 2/3	
	Location Purpose	
 	7S		Pipeline Segment	
	Pipeline Segment defined by 1 location [or first of 2 locations]	
 	IJ		Injection Point	
 	M2		Receipt Location	
 	MQ		Delivery Location	
 	MV		Mainline	
 	NQ		Pipeline Segment Boundary	
	Pipeline Segment defined by 2 locations [or second of 2 locations]	
 	SB		Storage Area	
 	WR		Withdrawal Point	
	N102	93	Name	X	1 	AN 1/60	
	Location Name

For NAESB WGQ, this data element is sender's option.	
Must Use	N103	66	Identification Code Qualifier	X	1 	ID 1/2	
 	DR		Gas Industry Standards Board (GISB) Data Reference Number (DRN)	
	For NAESB WGQ, this code value may only be used when sending the Location in N104.	
 	SV		Service Provider Number	
	For NAESB WGQ, this code value may only be used when sending the Location Proprietary Code in N104.	
Must Use	N104	67	Identification Code	X	1 	AN 2/17	
	Location/Location Proprietary Code

The data element maximum length is reduced from that which is specified in the ASC X12 standards.

	Segment:	LCD Place/Location Description
	Position:	1200
	Loop:	N1        Optional (Must Use)
	Level:	Detail
	Usage:	Optional
	Max Use:	1
Notes:		For NAESB WGQ, this segment is sender's option.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	LCD05	66	Identification Code Qualifier	X	1 	ID 1/2	
 	ZN		Zone	
Must Use	LCD06	67	Identification Code	X	1 	AN 2/80	
	Location Zone	

	Segment:	N9 Extended Reference Information
	Position:	1300
	Loop:	N1        Optional (Must Use)
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
Notes:		For NAESB WGQ, this segment is sender's option.	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	N901	128	Reference Identification Qualifier	M	1 	ID 2/3	
 	L1		Letters or Notes	
Must Use	N902	127	Reference Identification	X	1 	AN 1/80	
	Comments and Notes	

	Segment:	SE Transaction Set Trailer
	Position:	1600
	Loop:
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	    Attributes    
Must Use	SE01	96	Number of Included Segments	M	1 	N0 1/10	
Must Use	SE02	329	Transaction Set Control Number	M	1 	AN 4/9