Talking points/high level factors for CISS on Automated Checkout if members wants to continue working on this issue and wants CISS to provide guidance to industry on Automated Checkout.

1. Data exchange shall include NSI megawatt for agreed upon time interval, direction of power flow and three part communication recording method.
* These would be the things that you must need to be able to successfully checkout with your neighboring BA
1. Data exchanges may be additionally expanded for before-the-fact & after-the-fact daily checkouts in addition to Real-Time Checkouts.

- These would be the things that you may add to exchange additional data related to NSI

1. Two parties may need to establish new failure procedures and internal alarms when automating NSI.

- These would be the things that participating neighbors might want to consider in their failure scenarios.